*SUPER VALVE FLUSH*

**P.I.N. I-350 – 5GLP**

***SUPER***

***VALVE FLUSH***

|  |  |
| --- | --- |
| Health | 0 |
| Flammability | 1 |
| Reactivity | 0 |
| Personal | A |

**DIRECTIONS FOR USE:**

Apply ***Super Valve Flush*** using a rechargeable spray can or pour directly into opening. Allow product to sit for 5 minutes.

Dump out any residual product and let air dry. If the equipment allows blow out with air guns. Once completely dry begin applying new grease or lubricant.

Batch Number: #





**INTERNAL VALVE CLEANER**

REMOVES THE FOLLOWING:

**GREASE & LUBRICANTS**

**PREVIOUS BUILD UP OF SOLIDS**

**CONTAMINENTS**

**DEPOSITS**

**PREPARES FITTINGS AND INTERNALS FOR NEW GREASE**

Keep Out Of Reach of Children

**Net Contents**

**□** 5 GALLONS

**First Aid**

**Eye Irritation:** Flush with water. Consult physician and poison control immediately.

**Skin Contact:** wash skin with soap and water, if irritation occurs, call physician.

**Ingestion:** If swallowed be slightly toxic. Consult physician and poison control immediately.

Dispose of in accordance with local, state and federal regulations.





Warning: Harmful if inhaled. Avoid breathing dust/fumes/gas/mist/spray. Use only outdoors or in a well-ventilated area.