**DIESEL COOL ANTIFREEZE**

50/50 Blend is a ready to use extended life coolant for diesel engines. It is ideal for industrial applications. Provides trouble free performance in oil & gas, marine, and mixed fleet operations. Helps eliminate down time through our unique heat transfer technology.

**P.I.N. I-340-55D**

**Diesel Cool**

Batch Number: #







**Diesel Cool**

**ANTIFREEZE**

**50/50 Blend**

******

**Oxidation Stabilizers**

**Extend Service Life**

**Inhibits Rust & Corrosion**

**Enhanced with Anti-Wear Additives**

**Nitrate Free Formula**

**Resists Deposit Formation**

Keep Out Of Reach of Children

**Net Contents**

**□** 5 Gallons □ 20 Gallons

**□** 30 Gallons **□** 55 Gallons

**First Aid**

**Inhalation:** Remove to fresh air. If rapid recovery does not occur, transport to nearest medical facility for additional treatment.

**Eye Irritation:** Flush eye with copious amounts of water. If persistent irritation occurs, obtain medical attention.

**Skin Contact:** Remove contaminated clothing. Flush exposed area with water and follow by washing with soap if available. If persistent irritation occurs, obtain medical attention.

**Ingestion:** DO NOT DELAY. Do no induce vomiting: transport to nearest medical facility for additional treatment. If vomiting occurs spontaneously, keep head below hips to prevent aspiration.

Dispose of in accordance with local, state and federal regulations.



Warning: Harmful if inhaled. Avoid breathing dust/fumes/gas/mist/spray. Use only outdoors or in a well-ventilated area.