

Ready Wrap

Directions for Use:

Do Not Use on Any

Gas Lines, Fuel Lines, or Brake Lines

1. Clean surface.
2. Cut-off length to be used.
3. Keep wrap clean and dry.
4. Stretch out Ready Wrap while wrapping.
5. Overlap coverage onto itself to achieve adhesion.
6. For best results, stretch Ready Wrap twice its size for a faster, better bond.
7. Continue to wrap around area to be repaired by overlapping with each new wrap.
8. The first and last wrap should completely overlap for a complete bond.
9. Most repairs will require 3-5 layers and must be wrapped 2-5 inches on either side of the repair.

Ready Wrap is not reusable.

\*Additional wrap can be added to a repair at any time

[www.encoreindustrial.com](http://www.encoreindustrial.com)

281-944-4777 • 1-877-703-3044

**Encore Industrial Products, LLC**

**3502 Bacor Rd.**

**Houston, TX 77084**

[www.encoreindustrial.com](http://www.encoreindustrial.com)

281-944-4777 • 1-877-703-3044

**Encore Industrial Products, LLC**

**3502 Bacor Rd.**

**Houston, TX 77084**