**1” X 120” Roll**

A picture containing drawing

Description automatically generated

Ready Wrap

Self-Bonding Repair Wrap

[](https://www.google.com/url?sa=i&rct=j&q=&esrc=s&source=images&cd=&cad=rja&uact=8&ved=2ahUKEwjuxvuOxfbbAhUDZKwKHTI4AIkQjRx6BAgBEAU&url=https://aimdynamics.com/product/ul-listed-current-sensor-4lsf-sentran-corp/&psig=AOvVaw0XFWCCj3o-AiNOzFkhchAz&ust=1530281468407523)

**Insulates up to 400 volts/mil**

**Temperature safe to 500⁰F**

**Tensile Strength to 700 PSI**

**Creates an Air & Water Tight Seal**

**Directions for Use on Back**

**of Package**

Product Codes: **L-275 Black L-276 Purple L-277 Green L-278 Blue L-279 Brown**

**Warning:**

**Keep Out Of Reach of Children**

[www.encoreindustrial.com](http://www.encoreindustrial.com)

281-944-4777 • 1-877-703-3044

**Encore Industrial Products, LLC**

**3502 Bacor Rd.**

**Houston, TX 77084**